

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **AGRICULTURE AND RESOURCE DEVELOPMENT**  Petroleum Branch  360-1395 Ellice Ave, Winnipeg, MB R3G 3P2  **T** 204-945-6577 **F** 204-945-0586  [www.manitoba.ca](http://www.manitoba.ca) | | | | | | | |
| **WEEKLY WELL ACTIVITY REPORT** | | | | | | | |
|  |  |  | |  |  | |  |
| PETROLEUM INDUSTRY ACTIVITY REPORT | | | | | | | |
| (January 1/22 – January 10/22) | | | | | | | |
|  |  |  |  | | |  |  |
| **DRILLING ACTIVITY** | **To Jan 10/22** |  | **To Jan 11/21** | | |  | 2021 Total |
|  |  |  |  | | |  |  |
| Drilling Licences Issued | 0 |  | 0 | | |  | 178 |
| Licences Cancelled | 0 |  | 0 | | |  | 9 |
| Vertical Wells Drilled | 0 |  | 0 | | |  | 9 |
| Horizontal Wells Drilled | 6 |  | 0 | | |  | 164 |
| Stratigraphic Test Holes Drilled | 0 |  | 0 | | |  | 1 |
| Wells Drilled - Total | 6 |  | 0 | | |  | 174 |
| No. of Metres Drilled | 14 015 |  | 0 | | |  | 372 739 |
| Wells Re-entered | 0 |  | 0 | | |  | 6 |
| Wells Being Drilled | 3 |  | 3 | | |  | 0 |
| No. of Active Rigs | 5 |  | 3 | | |  | 0 |
| Wells Licenced but Not Spudded | -6 |  | 52 | | |  | 62 |
|  |  |  |  | | |  |  |
| Wells Completed as Potential Oil Wells | 6 |  | 0 | | |  | 168 |
| Wells Abandoned Dry | 0 |  | 0 | | |  | 3 |
| Wells Drilled but Not Completed | 0 |  | 0 | | |  | 0 |
| Other Completions | 0 |  | 0 | | |  | 3 |
|  |  |  |  | | |  |  |
| New Wells on Production | 0 |  | 0 | | |  | 34 |
|  |  |  |  | | |  |  |
| **GEOPHYSICAL ACTIVITY** |  |  |  | | |  |  |
|  |  |  |  | | |  |  |
| Geophysical Programs Licenced | 0 |  | 0 | | |  | 6 |
| Licences Cancelled | 0 |  | 0 | | |  | 0 |
| Kilometers Licenced | 0 |  | 0 | | |  | 439 |
| Kilometers Run | 0 |  | 0 | | |  | 438 |
|  |  |  |  | | |  |  |
|  | **2021** |  | **2020** | | |  |  |
| **OIL PRICES (Average)** | $/m3 ($/bbl) |  | $/m3 ($/bbl) | | |  |  |
|  |  |  |  | | |  |  |
| Month of November | 43 615.98 (97.88) |  | 303.27 (48.19) | | |  |  |
| Month of December | 43 615.98 (97.88) |  | 346.19 (55.01) | | |  |  |
|  |  |  |  | | |  |  |
| **OIL PRODUCTION (M3)** | **2021** |  | **2020** | | |  |  |
| Month of December | 190 750.2 |  | 179 854.0 | | |  |  |

**WEEKLY WELL ACTIVITY REPORT**

**10 January 2022**

|  |  |
| --- | --- |
| Lic. No.: 5104 | Routledge Unit No. 1 HZNTL WIW 9-29-9-25 (WPM)  **UWI: 102.12-28-009-25W1.00 - Leg #1 Revised**  UWI: 103.09-29-009-25W1.02  ***Please note revised Well Name and UWI as reflected in As-Drilled***  ***Well Name changed fr. 11-28-9-25 to 9-29-9-25***  ***UWI: 102.12-28-009-25W1.00 – Leg #1 Revised***  ***Licenced as: 102.11-28…Drilled as: 102.12-28*** |
| Lic. No.: 6542 | Routledge Unit No. 1 HZNTL WIW A9-29-9-25 (WPM)  **UWI:** **103.09-29-009-25W1.00 - Leg #1**  **UWI: 103.09-29-009-25W1.02 - Leg #2**  **Please note revised UWI** |
|  | **103.09-29-009-25W1.02 - Leg #2** |
| Lic. No.: 11428 | Whitewater Unit No. 2 HZNTL 13-2-3-21 (WPM)  **102.13-02-003-21W1.00 - Leg #1 Revised**  ***Please note revised Well Name and UWI as reflected in As-Drilled***  ***Well Name changed fr. 16-3-2-21 to 13-2-3-21***  ***UWI: 102.13-02-003-21W1.00 – Leg #1 Revised***  ***Licenced as 102.16-03…Drilled as 102.13-02*** |
| Lic. No.: 11519 | Routledge Unit No. 1 Prov. HZNTL 11-20-9-25 (WPM)  102.11-20-009-25W1.00 - Leg #1  **102.11-20-009-25W1.02 - Leg #2 Added**  **Please note added UWI**  **102.11-20-009-25W1.00 - Leg #1**  Spud Date: 04-Jan-2022  K.B. Elevation: 438.05 m  Surface Casing: 244.50 mm @ 142.00 m with 9.0 t  Intermediate Casing: 177.80 mm @ 821.00 m with 14.5 t  Finished Drilling: 07-Jan-2022  Total Depth: 1373.00 m |
|  | **102.11-20-009-25W1.02 - Leg #2**  Kick-Off Date: 08-Jan2022  Kick-Off Point: 914.00 m  Finished Drilling: 09-Jan-2022  Total Depth: 1923.00 m |
|  | **102.11-20-009-25W1.00 - Leg #1**  **102.11-20-009-25W1.02 - Leg #2**  Rig Released: 09-Jan-2022  Status: Waiting On Service Rig (WOSR)  Waiting On Service Rig: 09-Jan-2022 |
| Lic. No.: 11536 | Corex Virden HZNTL 4-17-9-25 (WPM)  UWI: 102.04-17-009-25W1.00  Status: Moving In Rotary Tools (MIRT)  Moving In Rotary Tools: 10-Jan-2022 |
| Lic. No.: 11544 | Corex Virden Prov. HZNTL 6-35-11-26 (WPM)  UWI: 100.06-35-011-26W1.00  Status: Completing (COMP)  Completing: 17-Dec-2021 |
| Lic. No.: 11546 | Melita Pierson HZNTL A13-21-2-28 (WPM)  **102.13-21-002-28W1.00 - Leg #1 Revised**  **100.14-21-002-28W1.02 - Leg #2 Revised**  ***Please note revised Well Name and UWI’s to reflect As Drilled:***  ***Well Name changed fr. 16-21-02-28 to 13-21-…*** |
|  | ***UWI: 102.13-21-002-28W1.00 - Leg #1 Revised***  ***Licenced as 100.16-21…Drilled as 102.13-21…***  ***UWI: 100.14-21-002-28W1.02 - Leg #2 Revised***  ***Licenced as 100.16-21…Drilled as 100.14-21…*** |
| Lic. No.: 11561 | Tundra et al Daly Sinclair HZNTL 13-16-8-28 (WPM)  102.13-16-008-28W1.00  **102.13-16-008-28W1.00 - Leg #1 Revised**  ***Please note revised Well Name and UWI’s to reflect As Drilled:***  ***Well Name changed fr. 04-21-02-28 to 13-16-…***  ***UWI: 102.13-16-002-28W1.00 - Leg #1 Revised***  ***Licenced as 103.04-21…Drilled as 102.13-16…*** |
| Lic. No.: 11575 | Tundra Whitewater HZNTL 8-8-3-21 (WPM)  100.08-08-003-21W1.00  **100.08-08-003-21W1.00 - Leg #1 Revised**  ***Please note revised Well Name and UWI’s to reflect As Drilled:***  ***Well Name changed fr. 01-08-03-21 to 08-08-…***  ***UWI: 100.08-08-003-21W1.00 - Leg #1 Revised***  ***Licenced as 100.01-08…Drilled as 100.08-08…*** |
| Lic. No.: 11576 | Tundra Whitewater HZNTL A8-8-3-21 (WPM)  102.08-08-003-21W1.00  **102.08-08-003-21W1.00 - Leg #1 Revised**  ***Please note revised Well Name and UWI’s to reflect As Drilled:***  ***Well Name changed fr. 01-08-03-21 to 08-08-…***  ***UWI: 102.08-08-003-21W1.00 - Leg #1 Revised***  ***Licenced as 102.01-08…Drilled as 102.08-08…*** |
| Lic. No.: 11629 | Tundra Daly Sinclair HZNTL D8-8-10-28 (WPM)  UWI: 107.08-08-010-28W1.00  Spud Date: 07-Jan-2022  K.B. Elevation: 519.13 m  Surface Casing: 244.50 mm @ 142.00 m with 6.5 t  Status: Drilling Ahead (DR)  Drilling Ahead: 10-Jan-2022 |
|  |  |
| Lic. No.: 11630 | Tundra Daly Sinclair HZNTL B8-7-10-28 (WPM)  UWI: 104.08-07-010-28W1.00  Finished Drilling: 05-Jan-2022  Total Depth: 2285.00 m  Production Casing: 139.70 mm @ 2285.00 m with 34.0 t  Rig Released: 06-Jan-2022 |
|  | Status: Waiting On Service Rig (WOSR)  Waiting On Service Rig: 06-Jan-2022 |
| Lic. No.: 11631 | Tundra Daly Sinclair HZNTL A8-8-10-29 (WPM)  UWI: 102.08-08-010-29W1.00  ***Please note revision to Report dated 22-Nov-2021***  ***Drilling Contractor: Ensign Drilling Inc. – Rig #12***  Spud Date: 04-Jan-2022  K.B. Elevation: 534.34 m  Surface Casing: 244.50 mm @ 142.00 m with 6.5 t  Finished Drilling: 08-Jan-2022  Total Depth: 2306.00 m  Production Casing: 139.70 mm @ 2306.00 m with 33.5.0 t  Rig Released: 09-Jan-2022 |
|  | Status: Waiting On Service Rig (WOSR)  Waiting On Service Rig: 09-Jan-2022 |
| Lic. No.: 11632 | Tundra Daly Sinclair HZNTL B12-8-10-29 (WPM)  UWI: 103.12-08-010-29W1.00  Spud Date: 06-Jan-2022  K.B. Elevation: 528.13 m  Surface Casing: 244.50 mm @ 144.00 m with 6.0 t  Finished Drilling: 09-Jan-2022  Total Depth: 2172.00 m  Production Casing: 139.70 mm @ 2172.00 m with 33.5 t  Rig Released: 10-Jan-2022 |
|  | Status: Waiting On Service Rig (WOSR)  Waiting On Service Rig: 10-Jan-2022 |
| Lic. No.: 11637 | Tundra Daly Sinclair HZNTL A9-32-10-28 (WPM)  UWI: 102.09-32-010-28W1.00  Intermediate Casing: 139.70 mm @ 892.63 m with 33.0 t  Finished Drilling: 07-Jan-2022  Total Depth: 2313.00 m  Rig Released: 07-Jan-2022 |
|  | Status: Waiting On Service Rig (WOSR)  Waiting On Service Rig: 07-Jan-2022 |
| Lic. No.: 11645 | Tundra Daly Sinclair Prov. HZNTL B8-6-9-28 (WPM)  UWI: 103.08-06-009-28W1.00  Spud Date: 09-Jan-2022  K.B. Elevation: 516.55 m  Surface Casing: 244.50 mm @ 144.00 m with 6.5 t  Status: Cementing Casing (CMT CSG)  Cementing Casing: 10-Jan-2022 |
|  |  |
| Lic. No.: 11658 | Melita Pierson HZNTL 13-22-2-28 (WPM)  UWI: 100.13-22-002-28W1.00 - Leg #1  UWI: 100.13-22-002-28W1.02 - Leg #2  **UWI: 100.13-22-002-28W1.00 – Leg #1**  Spud Date: 05-Jan-2022  K.B. Elevation: 466.45 m  Surface Casing: 244.50 mm @ 159.00 m with 12.0 t  Intermediate Casing: 177.80 mm @ 1111.00 m with 16.0 t |
|  | Status: Drilling Ahead (DR)  Drilling Ahead: 10-Jan-2022 |