|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| GovMB_Logo_cmyk   |  | | --- | |  | |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
| **Economic Development, Investment, Trade & Natural Resources** | | | |  |  |  |  |  |
| Petroleum Branch |  |  |  |  |  |  |  |  |
| 360-1395 Ellice Ave, Winnipeg, MB R3G 3P2 | |  |  |  |  |  |  |  |
| **T** 204-945-6577 **F** 204-945-0586 | |  |  |  |  |  |  |  |
| [www.manitoba.ca](http://www.manitoba.ca/) |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
| **WEEKLY WELL ACTIVITY REPORT** | | | | | | | | |
|  |  |  |  |  |  |  |  |  |
| PETROLEUM INDUSTRY ACTIVITY REPORT | | | | | | | | |
|  |  |  |  |  |  |  |  |  |
| (January 1/23 -- Nov 6/23) | | | | | | | | |
|  |  |  |  |  |  |  |  |  |
| **DRILLING ACTIVITY** | |  | **To Nov 6/23** |  |  | **To Nov 7/22** |  | **2022 Total** |
|  |  |  |  |  |  |  |  |  |
| Drilling Licences Issued |  |  | 143 |  |  | 185 |  | 222 |
| Licences Cancelled |  |  | 8 |  |  | 3 |  | 11 |
| Vertical Wells Drilled |  |  | 3 |  |  | 4 |  | 7 |
| Horizontal Wells Drilled |  |  | 135 |  |  | 185 |  | 220 |
| Stratigraphic Test Holes Drilled | |  | 1 |  |  | 0 |  | 1 |
| Wells Drilled - Total |  |  | 139 |  |  | 189 |  | 228 |
| No. of Metres Drilled |  | 307087 | |  | 429546 | |  | 503107 |
| Wells Re-entered |  |  | 0 |  |  | 6 |  | 7 |
| Wells Being Drilled |  |  | 1 |  |  | 4 |  | 0 |
| No. of Active Rigs |  |  | 1 |  |  | 4 |  | 0 |
| Wells Licenced but Not Spudded | |  | 42 |  |  | 54 |  | 46 |
|  |  |  |  |  |  |  |  |  |
| Wells Completed as Potential Oil Wells | |  | 136 |  |  | 186 |  | 221 |
| Wells Abandoned Dry |  |  | 3 |  |  | 0 |  | 1 |
| Wells Drilled but Not Completed | |  | 0 |  |  | 0 |  | 0 |
| Other Completions |  |  | 0 |  |  | 3 |  | 3 |
|  |  |  |  |  |  |  |  |  |
| New Wells on Production |  |  | 0 |  |  | 0 |  | 0 |
|  |  |  |  |  |  |  |  |  |
| **GEOPHYSICAL ACTIVITY** | |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
| Geophysical Programs Licenced | |  | 0 |  |  | 0 |  | 0 |
| Licences Cancelled |  |  | 0 |  |  | 0 |  | 0 |
| Kilometers Licenced |  |  | 0 |  |  | 0.00 |  | 0 |
| Kilometers Run |  |  | 0 |  |  | 0 |  | 0 |
|  |  |  |  |  |  |  |  |  |
|  |  |  | **2023** |  |  | **2022** |  |  |
| **OIL PRICES (Average)** |  | $/M3 | $/BBL | |  | $/M3 | $/BBL | |  |  |
|  |  |  |  |  |  |  |  |  |
| Month of September |  | 746.94 | 118.69 |  | 693.58 | 110.21 |  |  |
| Month of October |  | 656.24 | 104.28 |  | 708.50 | 112.58 |  |  |
|  |  |  |  |  |  |  |  |  |
| **OIL PRODUCTION (M3)** |  |  | **2023** |  |  | **2022** |  |  |
| Month of October |  | 190,536.3 | |  | 195,432.0 | |  |  |

**WEEKLY WELL ACTIVITY REPORT**

**06 November 2023**

|  |  |
| --- | --- |
| Lic. No.: 11955 | Routledge Unit No. 1 Prov. HZNTL 11-20-9-25 (WPM)  UWI: 103.11-20-009-25W1.00  Status: Moving In Rotary Tools (MIRT)  Moving In Rotary Tools: 06-Nov-2023 |
| Lic. No.: 11956 | Corex Virden Prov. HZNTL 13-20-9-25 (WPM)  UWI: 100.13-20-009-25W1.00  Spud Date: 02-Nov-2023  K.B. Elevation: 437.52 m  Surface Casing: 244.50 mm @ 146.00 m with 11.0 t  Intermediate Casing: 177.80 mm @ 802.00 m with 17.0 t  Finished Drilling: 06-Nov-2023  Total Depth: 2195.00 m  Rig Released: 06-Nov-2023 |
|  | Status: Waiting On Service Rig (WOSR)  Waiting On Service Rig: 06-Nov-2023 |
| Lic. No.: 11967 | Corex Virden HZNTL 13-5-10-25 (WPM)  UWI: 100.13-05-010-25W1.00  Finished Drilling: 31-Oct-2023  Total Depth: 2356.00 m  Rig Released: 01-Nov-2023  Status: Waiting On Service Rig (WOSR)  Waiting On Service Rig: 01-Nov-2023 |
|  |  |
| Lic. No.: 12021 | Tundra Waskada WSW A16-21-1-25 (WPM)  UWI: 104.16-21-001-25W1.00  Spud Date: 04-Nov-2023  K.B. Elevation: 475.82 m  Surface Casing: 244.50 mm @ 145.00 m with 6.5 t  Finished Drilling: 05-Nov-2023  Total Depth: 727.00 m  Production Casing: 177.80 mm @ 727.00 m with 12.0 t  Rig Released: 06-Nov-2023 |
|  | Status: Waiting On Service Rig (WOSR)  Waiting On Service Rig: 06-Nov-2023 |
| Lic. No.: 12024 | Sinclair Unit No. 1 HZNTL A5-20-8-29 (WPM)  UWI: 103.05-20-008-29W1.00  Status: Completing (COMP)  Completing: 01-Nov-2023 |
| Lic. No.: 12025 | Sinclair Unit No. 2 HZNTL A9-8-7-28 (WPM)  UWI: 103.09-08-007-28W1.00  Status: Completing (COMP)  Completing: 02-Nov-2023 |
| Lic. No.: 12028 | Tundra Pierson HZNTL 7-17-1-27 (WPM)  UWI: 100.07-17-001-27W1.00  Finished Drilling: 03-Nov-2023  Total Depth: 3346.00 m  Production Casing: 139.70 mm @ 3346.00 m with 46.0 t  Rig Released: 04-Nov-2023 |
|  | Status: Waiting On Service Rig (WOSR)  Waiting On Service Rig: 04-Nov-2023 |
| Lic. No.: 12035 | Sinclair Unit No. 1 HZNTL B13-8-8-29 (WPM)  UWI: 104.13-08-008-29W1.00  Finished Drilling: 01-Nov-2023  Total Depth: 2685.00 m  Production Casing: 139.70 mm @ 2685.00 m with 44.3 t  Rig Released: 02-Nov-2023 |
|  | Status: Waiting On Service Rig (WOSR)  Waiting On Service Rig: 02-Nov-2023 |
| Lic. No.: 12036 | Sinclair Unit No. 11 HZNTL 14-35-7-29 (WPM)  UWI: 102.14-35-007-29W1.00  Spud Date: 03-Nov-2023  K.B. Elevation: 526.21 m  Surface Casing: 244.50 mm @ 142.00 m with 7.0 t |
|  | Status: Drilling Ahead (DR)  Drilling Ahead: 06-Nov-2023 |
| Lic. No.: 12040 | Tundra Waskada HZNTL 11-1-2-25 (WPM)  UWI: 100.11-01-002-25W1.00  Licence Issued: 02-Nov-2023  Licensee: Tundra Oil & Gas Limited  Mineral Rights: Tundra Oil & Gas Limited  Contractor: Ensign Drilling Inc. - Rig# 10  Surface Location: 8D-3-2-25  Co-ords: 706.81 m N of S of Sec 3  201.07 m W of E of Sec 3  Grd Elev: 472.67 m  Proj. TD: 3363.10 m (Triassic)  Field: Waskada  Classification: Non Confidential Development  Status: Location(LOC) |
| Lic. No.: 12041 | Ewart Unit No. 3 et al Prov. HZNTL E13-29-8-28 (WPM)  UWI : 106.13-29-008-28W1.00  Licence Issued: 02-Nov-2023  Licensee: Tundra Oil & Gas Limited  Mineral Rights: Tundra Oil & Gas Limited  Contractor: Ensign - Trinidad Drilling Inc. - Rig# 9  Surface Location: 13C-28-8-28  Co-ords: 46.00 m S of N of Sec 28  104.32 m E of W of Sec 28  Grd Elev: 497.41 m  Proj. TD: 2462.50 m (Devonian)  Field: Daly Sinclair  Classification: Non Confidential Development  Status: Location(LOC) |