|  |
| --- |
|  |
| Petroleum Branch360-1395 Ellice Ave, Winnipeg, MB R3G 3P2**T** 204-945-6577 **F** 204-945-0586[www.manitoba.ca](http://www.manitoba.ca) |
| **WEEKLY WELL ACTIVITY REPORT** |
|  |  |  |  |  |  |
|  PETROLEUM INDUSTRY ACTIVITY REPORT |
|  (January 1/20 – February 3/20) |
|  |  |  |  |  |  |
| **DRILLING ACTIVITY** | **To February 3/20** |  | To February 4/19 |  | 2019 Total |
|  |  |  |  |  |  |
| Drilling Licences Issued | 21 |  | 22 |  | 225 |
| Licences Cancelled | 0 |  | 2 |  | 17 |
| Vertical Wells Drilled | 0 |  | 1 |  | 13 |
| Horizontal Wells Drilled | 29 |  | 38 |  | 208 |
| Stratigraphic Test Holes Drilled | 0 |  | 0 |  | 0 |
| Wells Drilled - Total | 29 |  | 39 |  | 221 |
| No. of Metres Drilled | 67 623 |  | 84 489 |  | 482 956 |
| Wells Re-entered | 0 |  | 0 |  | 1 |
| Wells Being Drilled | 4 |  | 3 |  | 0 |
| No. of Active Rigs | 5 |  | 7 |  | 7 |
| Wells Licenced but Not Spudded | 47 |  | 53 |  | 58 |
|  |  |  |  |  |  |
| Wells Completed as Potential Oil Wells | 29 |  | 38 |  | 217 |
| Wells Abandoned Dry | 0 |  | 0 |  | 1 |
| Wells Drilled but Not Completed | 0 |  | 0 |  | 0 |
| Other Completions | 0 |  | 1 |  | 4 |
|  |  |  |  |  |  |
| New Wells on Production | 0 |  | 0 |  | 32 |
|  |  |  |  |  |  |
| **GEOPHYSICAL ACTIVITY** |  |  |  |  |  |
|  |  |  |  |  |  |
| Geophysical Programs Licenced | 0 |  | 1 |  | 4 |
| Licences Cancelled | 0 |  | 0 |  | 1 |
| Kilometers Licenced  | 0 |  | 20 |  | 580 |
| Kilometers Run | 79  |  | 0 |  | 20 |
|  |  |  |  |  |  |
|  | **2019** |  | **2018** |  |  |
| **OIL PRICES (Average)** | $/m3 ($/bbl) |  | $/m3 ($/bbl) |  |  |
|  |  |  |  |  |  |
| Month of November |  443.23 (70.43) |  |  347.77 (55.26) |  |  |
| Month of December | 43 430.96 (68.48) |  |  259.97 (41.31) |  |  |
|  |  |  |  |  |  |
| **OIL PRODUCTION (M3)** | **2018** |  | **2017** |  |  |
| Month of August | 189 804.4 |  | 193 117.8 |  |  |

**WEEKLY WELL ACTIVITY REPORT**

**03 February 2020**

|  |  |
| --- | --- |
| Lic. No.: 5259 | Tundra Daly Sinclair Prov. **OBS** 2-28-9-29 (WPM)**UWI: 100.02-28-009-29W1.00****UWI: 100.02-28-009-29W1.02 - Added****Please note added UWI and change in Well Name****UWI: 100.02-28-009-29W1.00**Status: Abandoned Producer (ABD P)Abandoned Producer: 14-Jun-2019**UWI: 100.02-28-009-29W1.02**Status: Completing (COMP)Completing: 30-Jul-2019 |
|  |  |
| Lic. No.: 11238 | Corex Virden HZNTL A13-26-10-26 (WPM)UWI: 103.13-26-010-26W1.00 - Leg #1UWI: 103.13-26-010-26W1.02 - Leg #2Status: Completing (COMP)Completing: 03-Feb-2020 |
|  |  |
| Lic. No.: 11258 | South Pierson Unit No. 1 HZNTL 15-17-2-29 (WPM)UWI: 102.15-17-002-29W1.00 ***Please note revision to Report dated 27-May-2019:******Drilling Contractor: Stampede Drilling Inc.– Rig #7***Status: Moving In Rotary Tools (MIRT)Moving In Rotary Tools: 03-Feb-2020 |
| Lic. No.: 11333 | South Pierson Unit No. 2 Prov. HZNTL B3-20-2-29 (WPM)UWI: 103.03-20-002-29W1.00 Status: Completing (COMP)Completing: 02-Feb-2020 |
| Lic. No.: 11334 | South Pierson Unit No. 2 HZNTL A4-19-2-29 (WPM)UWI: 103.04-19-002-29W1.00 Status: Completing (COMP)Completing: 03-Feb-2020 |
| Lic. No.: 11335 | South Pierson Unit No. 1 HZNTL 13-17-2-29 (WPM)UWI: 100.13-17-002-29W1.00 Finished Drilling: 28-Jan-2020Total Depth: 2071.00 mIntermediate Casing: 139.70 mm @ 2071.00 m with 47.6 tRig Released: 28-Jan-2020Status: Waiting On Service Rig (WOSR)Waiting On Service Rig: 28-Jan-2020 |
|  |  |
| Lic. No.: 11336 | South Pierson Unit No. 1 HZNTL A13-17-2-29 (WPM)UWI: 102.13-17-002-29W1.00 - Leg #1***Please note revision to Report dated 09-Sep-2019:******Drilling Contractor: Stampede Drilling Inc.– Rig #7***Spud Date: 29-Jan-2020K.B. Elevation: 480.95 mSurface Casing: 244.50 mm @ 160.00 m with 13.0 tFinished Drilling: 01-Feb-2020Total Depth: 1920.00 mIntermediate Casing: 139.70 mm @ 1920.00 m with 44.0 t Rig Released: 02-Feb-2020 |
|  | Status: Waiting On Service Rig (WOSR)Waiting On Service Rig: 02-Feb-2020 |
| Lic. No.: 11339 | Virden Roselea Unit No. 3 HZNTL 3-23-10-26 (WPM)UWI: 102.03-23-010-26W1.00 - Leg #1UWI: 102.03-23-010-26W1.02 - Leg #2UWI: 102.03-23-010-26W1.00 - Leg #1Spud Date: 29-Jan-2020K.B. Elevation: 443.55 mSurface Casing: 244.50 mm @ 175.00 m with 12.0 tIntermediate Casing: 177.80 mm @ 868.00 m with 13.0 tFinished Drilling: 02-Feb-2020Total Depth: 1777.00 mUWI: 102.03-23-010-26W1.02 - Leg #2Kick-Off Date: 02-Feb-2020Kick-Off Point: 908.00 mStatus: Drilling Ahead (DR)Drilling Ahead: 03-Feb-2020 |
| Lic. No.: 11342 | Sinclair Unit No. 17 HZNTL B9-19-8-28 (WPM)UWI: 103.09-19-008-28W1.00 Status: Completing (COMP)Completing: 28-Jan-2020 |
| Lic. No.: 11358 | North Virden Scallion Unit No. 1 HZNTL 8-21-11-26 (WPM)UWI: 102.08-21-011-26W1.00 Intermediate Casing: 177.80 mm @ 768.00 m with 11.3 tFinished Drilling: 29-Jan-2020Total Depth: 1540.00 mRig Released: 29-Jan-2020 |
|  | Status: Waiting On Service Rig (WOSR)Waiting On Service Rig: 29-Jan-2020 |
| Lic. No.: 11366 | Tundra Virden 13-13-11-27 (WPM)UWI: 100.13-13-011-27W1.00***Please note revision to Report dated 25-Nov-2019:******Drilling Contractor: Ensign Drilling Inc. – Rig #12***Spud Date: 01-Feb-2020K.B. Elevation: 479.51 mSurface Casing: 177.80 mm @ 137.00 m with 7.0 t |
|  | Status: Coring (COR)Coring: 03-Feb-2020 |
| Lic. No.: 11369 | Ewart Unit No. 11 Prov. HZNTL B9-16-8-28 (WPM)UWI: 103.09-16-008-28W1.00 Status: Completing (COMP)Completing: 02-Feb-2020 |
| Lic. No.: 11370 | Ewart Unit No. 11 Prov. HZNTL C16-16-8-28 (WPM)UWI: 104.16-16-008-28W1.00 Status: Completing (COMP)Completing: 03-Feb-2020 |
| Lic. No.: 11377 | Tundra Daly Sinclair HZNTL A12-8-10-29 (WPM)UWI: 102.12-08-010-29W1.00 Status: Completing (COMP)Completing: 31-Jan-2020 |
| Lic. No.: 11378 | Daly Unit No. 4 HZNTL 7-35-9-28 (WPM)UWI: 102.07-35-009-28W1.00Status: Completing (COMP)Completing: 01-Jan-2020 |
| Lic. No.: 11381 | Tundra Daly Sinclair HZNTL 16-34-9-28 (WPM)UWI: 102.16-34-009-28W1.00 Finished Drilling: 28-Jan-2020Total Depth: 3179.00 mIntermediate Casing: 139.70 mm @ 3179.00 m with 49.0 t Rig Released: 29-Jan-2020 |
|  | Status: Waiting On Service Rig (WOSR)Waiting On Service Rig: 29-Jan-2020 |
| Lic. No.: 11395 | Tundra Daly Sinclair HZNTL B8-12-9-29 (WPM)UWI: 103.08-12-009-29W1.00 Status: Completing (COMP)Completing: 28-Jan-2020 |
| Lic. No.: 11396 | Tundra Daly Sinclair HZNTL B8-29-9-29 (WPM)UWI: 104.08-29-009-29W1.00 Finished Drilling: 27-Jan-2020Total Depth: 2217.00 mIntermediate Casing: 139.70 mm @ 2217.00 m with 33.0 tRig Released: 28-Jan-2020Status: Waiting On Service Rig (WOSR)Waiting On Service Rig: 28-Jan-2020 |
| Lic. No.: 11402 | Cromer Unit No. 2 HZNTL 9-23-9-28 (WPM)UWI: 100.09-23-009-28W1.00 Spud Date: 29-Jan-2020K.B. Elevation: 499.35 mSurface Casing: 244.50 mm @ 141.00 m with 7.5 tFinished Drilling: 31-Jan-2020Total Depth: 2140.00 mIntermediate Casing: 139.70 mm @ 2140.00 m with 35.0 tRig Released: 01-Feb-2020 |
|  | Status: Waiting On Service Rig (WOSR)Waiting On Service Rig: 01-Feb-2020 |
| Lic. No.: 11408 | Tundra Pierson Prov. HZNTL 7-20-2-29 (WPM)UWI: 100.07-20-002-29W1.00 Spud Date: 30-Jan-2020K.B. Elevation: 478.46 mSurface Casing: 219.10 mm @ 138.00 m with 6.0 tFinished Drilling: 01-Feb-2020Total Depth: 1698.00 mIntermediate Casing: 139.70 mm @ 1698.00 m with 26.0 tRig Released: 02-Feb-2020 |
|  | Status: Waiting On Service Rig (WOSR)Waiting On Service Rig: 02-Feb-2020 |
| Lic. No.: 11409 | Tundra Pierson Prov. HZNTL A15-16-1-27 (WPM)UWI: 102.15-16-001-27W1.00 Spud Date: 02-Feb-2020K.B. Elevation: 456.29 mSurface Casing: 219.10 mm @ 136.00 m with 6.0 tStatus: Drilling Ahead (DR)Drilling Ahead: 03-Feb-2020 |
|  |  |
| Lic. No.: 11413 | Tundra Daly Sinclair HZNTL A9-23-10-29 (WPM)UWI: 102.09-23-010-29W1.00 ***Please note revision to Report dated 20-Jan-2020:******Drilling Contractor: Ensign Drilling Inc. – Rig #12***Spud Date: 28-Jan-2020K.B. Elevation: 528.84 mSurface Casing: 244.50 mm @ 136.00 m with 7.5 tFinished Drilling: 31-Jan-2020Total Depth: 2144.00 mIntermediate Casing: 177.80 mm @ 2144.00 m with 32.0 t Rig Released: 01-Feb-2020Status: Waiting On Service Rig (WOSR)Waiting On Service Rig: 01-Feb-2020  |
|  |  |
| Lic. No.: 11416 | Tundra Daly Sinclair HZNTL B16-13-9-29 (WPM)UWI: 103.16-13-009-29W1.00 Spud Date: 01-Feb-2020K.B. Elevation: 527.80 mSurface Casing: 244.50 mm @ 145.00 m with 7.5 tStatus: Drilling Ahead (DR)Drilling Ahead: 03-Feb-2020 |
|  |  |
| Lic. No.: 11419 | Goodlands Unit No. 2 HZNTL 2-6-1-24 (WPM)UWI:100.02-06-001-24W1.00Licence Issued: 03-Feb-2020Licensee: Tundra Oil & Gas LimitedMineral Rights: Tundra Oil & Gas LimitedContractor: Ensign - Trinidad Drilling Inc. - Rig# 9Surface Location: 4C-5-1-24Co-ords: 304.00 m N of S of Sec 5 170.00 m E of W of Sec 5Grd Elev: 482.65 mProj. TD: 1653.70 m (Triassic)Field: WaskadaClassification: Non Confidential DevelopmentStatus: Location(LOC) |
| Lic. No.: 11420 | Tundra Daly Sinclair Prov. HZNTL A16-16-10-28 (WPM)UWI:102.16-16-010-28W1.00Licence Issued: 03-Feb-2020Licensee: Tundra Oil & Gas LimitedMineral Rights: Tundra Oil & Gas LimitedContractor: Ensign Drilling Inc. - Rig# 12Surface Location: 16D-17-10-28Co-ords: 164.17 m S of N of Sec 17 72.50 m W of E of Sec 17Grd Elev: 512.12 mProj. TD: 2240.80 m (Mississippian)Field: Daly SinclairClassification: Non Confidential DevelopmentStatus: Location(LOC) |
|  |  |